#### CONTROL OF HAZARDOUS ENERGY SOURCES

**( LOCKOUT/TAGOUT )**

####  INSPECTION CERTIFICATION

#### DATE:

#### INSPECTOR:

SIGNATURE:

#### Machine or Equipment on Which Lockout/Tagout

#### Procedures Were Performed

Employee(s) Performing the Lockout/Tagout Procedures

**Employees Name (Please Print)** **Employee Signature**

Were all the lockout/tagout procedures performed correctly?

Yes \_\_\_\_\_ No \_\_\_\_\_

Comment on improper use of lockout/tagout procedures being used on the reverse side of this sheet (e.g., list of improper procedures being used which require retraining for the employee or notification of the procedures).

#### CONTROL OF HAZARDOUS ENERGY SOURCES

**( LOCKOUT/TAGOUT )**

##### EMPLOYEE TRAINING CERTIFICATION

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DATE: |  |  |  | AUTHORIZED EMPLOYEE |
|  |  |  |  |  | AFFECTED EMPLOYEE |
|  |  |  |  |  | OTHER EMPLOYEE |
| INSTRUCTOR: |  |  |  |
| SIGNATURE: |  |  |  |
| EMPLOYEE NAME (Please Print) |  | EMPLOYEE SIGNATURE |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

 **Lockout/Tagout Quiz**

1. A Lockout Device is a device that positively prevents a machine from being:

A) Started up

B) Becoming electrically energized

C) Turned on

D) All of the above

2. The employees that need LO/TO Training are?

A) Authorized Employees

B) Affected Employees

C) Other employees

D) All of the Above

3. OSHA requires that employers establish a “written energy control program”.

A) True

B) False

4. “Lockout” means “the placement of a tagout device on an energy-isolating device to indicate that the device and the equipment being controlled may not be operated until the tagout device is removed.”

A) True

B) False

5. The Cal/OSHA Standard that covers “The control of Hazardous Energy” is:

A) Title 8, Section 3314

B) Title 8, Section 2200

C) Title 8, Section 2739

D) Title 8, Section 2751

6. A “tagout device” is a device that uses a positive mean such as a lock to hold an energy-isolating device in a safe position and prevent the energizing of a machine or equipment.

A) True

B) False

7. “Affected employees” are those responsible for implementing the energy-control procedures or performing the service or maintenance activities.

A) True

B) False

8) Which statement is true concerning tagout devices?

A) Tags are only warning devices

B) Tagout devices can always be used in place of lockout devices

C) Tags may be removed by affected employees once LOTO is complete

D) Tags provide equivalent security to using a lock

9) LOTO devices must be labeled to identify the specific employees authorized to apply & remove them.

A) True

B) False

10) Employers must provide LOTO training specific to the needs of four types of employees: “Certified”, “Authorized”, “Affected” and “Other.”

A) True

B) False

**Lockout/Tagout Quiz Answers**

1. A Lockout Device is a device that positively prevents a machine from being:

A) Started up

B) Becoming electrically energized

C) Turned on

**D) All of the above**

2. The employees that need LO/TO Training are?

A) Authorized Employees

B) Affected Employees

C) Other employees

**D) All of the Above**

3. OSHA requires that employers establish a “written energy control program”.

**C) True**

D) False

4. “Lockout” means “the placement of a tagout device on an energy-isolating device to indicate that the device and the equipment being controlled may not be operated until the tagout device is removed.”

C) True

**D) False**

5. The OSHA Standard that covers “The control of Hazardous Energy” is:

**A) Title 8, Section 3314**

B) Title 8, Section 2200

C) Title 8, Section 2739

D) Title 8, Section 2751

6. A “tagout device” is a device that uses a positive mean such as a lock to hold an energy-isolating device in a safe position and prevent the energizing of a machine or equipment.

C) True

**D) False**

7. “Affected employees” are those responsible for implementing the energy-control procedures or performing the service or maintenance activities.

C) True

**D) False**

8) Which statement is true concerning tagout devices?

**A) Tags are only warning devices**

B) Tagout devices can always be used in place of lockout devices

C) Tags may be removed by affected employees once LOTO is complete

D) Tags provide equivalent security to using a lock

9) LOTO devices must be labeled to identify the specific employees authorized to apply & remove them.

**A) True**

B) False

10) Employers must provide LOTO training specific to the needs of four types of employees: “Certified”, “Authorized”, “Affected” and “Other”.

A) True

**B) False**